Next Previous Contents

## 7. DIO implementation

The Atari supports disk drives with either 128 or 256 byte sectors. The first three sectors of any disk are always 128 bytes long though. This is because the system can only boot from 128 bytes sectors.

Therefore the DIO read and write functions transfer only 128 bytes for sectors 1 to 3, regardless of the type of diskette.

Next Previous Contents