Next Previous Contents

## 7. Other hints

## 7.1 Interrupts

The runtime for the Atmos uses routines marked as `.CONDES` type 2 for interrupt handlers. Such routines must be written as simple machine language subroutines and will be called automatically by the interrupt handler code when they are linked into a program. See the discussion of the `.CONDES` feature in the assembler manual.

Next Previous Contents